**AES/PoUS**

**TECHNICAL SPECIFICATION XML (public)**

**(AES\_POUS\_SXML\_PL)**

***List of changes introduced in version 1.04.003***

| **Lp.** | **Miejsce zmiany** | **Opis** |
| --- | --- | --- |
|  | IEP01  IEP03 | Typos and numbering correction. |
|  | R0017S | The rule R0017S is added with the following content:  IF AdditionalInformation/code = '98200' is applicable for all goods items  THEN  it must be used at the GoodsShipmentForT2LT2LF level  to message IEP01 to item \*/GoodsItemForT2LT2LF/AdditionalInformation |
|  | R0018S | The rule R0018S is added with the following content:  IF \*/AdditionalInformationPL/Kod contain 'PCS01'  AND \*/AdditionalInformationPL/Opis contain IDSISC  THEN  The IDSISC is checked in the PDR 4003V1 code list AND must be active  AND must have a communication channel to send a message to PPCS.  to message IEP01 to items \*/GoodsItemForT2LT2LF/AdditionalInformationPL/Kod and \*/ GoodsShipmentForT2LT2LF/AdditionalInformationPL/Opis |
|  |  | Adding the suffix ‘POUS’ to the code list names.. |